** TagInfo scan (version 4.25.4) 2022-03-17 15:45:55 **
Report Type: -- IC INFO ------------------------------

# IC manufacturer:
HID Global

# IC type:
Unknown IC implementing ISO/IEC 14443-4

# NFC Forum NDEF-compliant tag:
Type 4 Tag

# Application information:
Type 4 Tag v2 application present

-- NDEF ------------------------------

# NFC data set information:
NDEF message containing 1 record
Current message size: 88 bytes
Maximum message size: 88 bytes
NFC data set access: Read-Only

# Record #1: URI record:
Type Name Format: NFC Forum well-known type (1)
Short Record
type: "U"
protocol field: https:// (0x04)
URI field: ebay.mtag.io/nh02?tagID=3D4C010E4051A5&tac=61BEB029711305D6CA55FE243F3708D3CDC14C6E
Payload length: 84 bytes
Payload data:

[00] 04 65 62 61 79 2E 6D 74 61 67 2E 69 6F 2F 6E 68 |␄ebay.mtag.io/nh|

[10] 30 32 3F 74 61 67 49 44 3D 33 44 34 43 30 31 30 |02?tagID=3D4C010|

[20] 45 34 30 35 31 41 35 26 74 61 63 3D 36 31 42 45 |E4051A5&tac=61BE|

[30] 42 30 32 39 37 31 31 33 30 35 44 36 43 41 35 35 |B029711305D6CA55|

[40] 46 45 32 34 33 46 33 37 30 38 44 33 43 44 43 31 |FE243F3708D3CDC1|

[50] 34 43 36 45                                     |4C6E            |


# NDEF message:
[00] D1 01 54 55 04 65 62 61 79 2E 6D 74 61 67 2E 69 |.␁TU␄ebay.mtag.i|

[10] 6F 2F 6E 68 30 32 3F 74 61 67 49 44 3D 33 44 34 |o/nh02?tagID=3D4|

[20] 43 30 31 30 45 34 30 35 31 41 35 26 74 61 63 3D |C010E4051A5&tac=|

[30] 36 31 42 45 42 30 32 39 37 31 31 33 30 35 44 36 |61BEB029711305D6|

[40] 43 41 35 35 46 45 32 34 33 46 33 37 30 38 44 33 |CA55FE243F3708D3|

[50] 43 44 43 31 34 43 36 45                         |CDC14C6E        |


# Capability Container (CC) file content:
Mapping version 2.0
CC length: 15 bytes
Maximum Le value: 256 bytes (0x100)
Maximum Lc value: 255 bytes (0xFF)
NDEF File Control TLV:
* Length: 6 bytes
* NDEF file ID: 0xE104
* Maximum NDEF data size: 90 bytes (0x5A)
* NDEF access: Read-Only (0x00FF)
[0] 00 0F 20 01 00 00 FF 04 06 E1 04 00 5A 00 FF    |␀␏␠␁␀␀.␄␆.␄␀Z␀. |


# Type 4 Tag File Control Information (FCI):
Type 4 Tag v2 application FCI: [none]
CC file FCI: [none]
NDEF file FCI: [none]

# NDEF file contents:
[00] 00 58 D1 01 54 55 04 65 62 61 79 2E 6D 74 61 67 |␀X.␁TU␄ebay.mtag|

[10] 2E 69 6F 2F 6E 68 30 32 3F 74 61 67 49 44 3D 33 |.io/nh02?tagID=3|

[20] 44 34 43 30 31 30 45 34 30 35 31 41 35 26 74 61 |D4C010E4051A5&ta|

[30] 63 3D 34 33 33 32 43 35 32 32 36 41 31 39 45 43 |c=4332C5226A19EC|

[40] 42 41 38 31 42 45 42 36 43 30 33 42 37 31 37 37 |BA81BEB6C03B7177|

[50] 42 33 35 46 37 36 35 31 46 33                   |B35F7651F3      |


-- EXTRA ------------------------------

# TagInfo Version:
Version :4.25.4

# Device Info:
Device Model :Google ( Pixel 4 XL )
Android OS Version :12

-- FULL SCAN ------------------------------

# Technologies supported:
ISO/IEC 7816-4 compatible
ISO/IEC 14443-4 (Type A) compatible
ISO/IEC 14443-3 (Type A) compatible


# Android technology information:
Tag description:
* TAG: Tech [android.nfc.tech.IsoDep, android.nfc.tech.NfcA, android.nfc.tech.Ndef]
* Maximum transceive length: 65279 bytes
* Default maximum transceive time-out: 618 ms
* Extended length APDUs supported
* Maximum transceive length: 253 bytes
* Default maximum transceive time-out: 618 ms
MIFARE Classic support present in Android

# Detailed protocol information:
ID: 3D:4C:01:0E:40:51:A5
ATQA: 0x4100
SAK: 0x20
ATS: 0x0578779002
* Max. accepted frame size: 256 bytes (FSCI: 8)
* Supported receive rates:
	- 106, 212, 424, 848 kbit/s (DR: 1, 2, 4, 8)
* Supported send rates:
	- 106, 212, 424, 848 kbit/s (DS: 1, 2, 4, 8)
* Different send and receive rates supported
* SFGT: 302.0 us  (SFGI: 0)
* FWT: 154.7 ms  (FWI: 9)
* NAD not supported
* CID supported
* Historical bytes: [none]

--------------------------------------

