** TagInfo scan (version 4.25.4) 2022-03-17 15:45:44 **
Report Type: -- IC INFO ------------------------------

# IC manufacturer:
Unknown manufacturer

# IC type:
Unknown IC implementing ISO/IEC 14443-4

# NFC Forum NDEF-compliant tag:
Type 4 Tag

# Application information:
Type 4 Tag v2 application present

-- NDEF ------------------------------

# NFC data set information:
NDEF message containing 1 record
Current message size: 88 bytes
Maximum message size: 88 bytes
NFC data set access: Read-Only

# Record #1: URI record:
Type Name Format: NFC Forum well-known type (1)
Short Record
type: "U"
protocol field: https:// (0x04)
URI field: ebay.mtag.io/nh02?tagID=3D4C010E4083A1&tac=27F347815A9B5FB8D92BCC323FB40B5A8688827A
Payload length: 84 bytes
Payload data:

[00] 04 65 62 61 79 2E 6D 74 61 67 2E 69 6F 2F 6E 68 |␄ebay.mtag.io/nh|

[10] 30 32 3F 74 61 67 49 44 3D 33 44 34 43 30 31 30 |02?tagID=3D4C010|

[20] 45 34 30 38 33 41 31 26 74 61 63 3D 32 37 46 33 |E4083A1&tac=27F3|

[30] 34 37 38 31 35 41 39 42 35 46 42 38 44 39 32 42 |47815A9B5FB8D92B|

[40] 43 43 33 32 33 46 42 34 30 42 35 41 38 36 38 38 |CC323FB40B5A8688|

[50] 38 32 37 41                                     |827A            |


# NDEF message:
[00] D1 01 54 55 04 65 62 61 79 2E 6D 74 61 67 2E 69 |.␁TU␄ebay.mtag.i|

[10] 6F 2F 6E 68 30 32 3F 74 61 67 49 44 3D 33 44 34 |o/nh02?tagID=3D4|

[20] 43 30 31 30 45 34 30 38 33 41 31 26 74 61 63 3D |C010E4083A1&tac=|

[30] 32 37 46 33 34 37 38 31 35 41 39 42 35 46 42 38 |27F347815A9B5FB8|

[40] 44 39 32 42 43 43 33 32 33 46 42 34 30 42 35 41 |D92BCC323FB40B5A|

[50] 38 36 38 38 38 32 37 41                         |8688827A        |


# Capability Container (CC) file content:
Mapping version 2.0
CC length: 15 bytes
Maximum Le value: 256 bytes (0x100)
Maximum Lc value: 255 bytes (0xFF)
NDEF File Control TLV:
* Length: 6 bytes
* NDEF file ID: 0xE104
* Maximum NDEF data size: 90 bytes (0x5A)
* NDEF access: Read-Only (0x00FF)
[0] 00 0F 20 01 00 00 FF 04 06 E1 04 00 5A 00 FF    |␀␏␠␁␀␀.␄␆.␄␀Z␀. |


# Type 4 Tag File Control Information (FCI):
Type 4 Tag v2 application FCI: [none]
CC file FCI: [none]
NDEF file FCI: [none]

# NDEF file contents:
[00] 00 58 D1 01 54 55 04 65 62 61 79 2E 6D 74 61 67 |␀X.␁TU␄ebay.mtag|

[10] 2E 69 6F 2F 6E 68 30 32 3F 74 61 67 49 44 3D 33 |.io/nh02?tagID=3|

[20] 44 34 43 30 31 30 45 34 30 38 33 41 31 26 74 61 |D4C010E4083A1&ta|

[30] 63 3D 30 30 38 31 33 33 34 45 37 41 38 34 42 35 |c=0081334E7A84B5|

[40] 37 31 35 43 46 34 46 42 36 31 36 39 42 30 39 43 |715CF4FB6169B09C|

[50] 43 37 43 34 32 34 34 37 36 37                   |C7C4244767      |


-- EXTRA ------------------------------

# TagInfo Version:
Version :4.25.4

# Device Info:
Device Model :Google ( Pixel 4 XL )
Android OS Version :12

-- FULL SCAN ------------------------------

# Technologies supported:
ISO/IEC 7816-4 compatible
ISO/IEC 14443-4 (Type A) compatible
ISO/IEC 14443-3 (Type A) compatible


# Android technology information:
Tag description:
* TAG: Tech [android.nfc.tech.IsoDep, android.nfc.tech.NfcA, android.nfc.tech.Ndef]
* Maximum transceive length: 65279 bytes
* Default maximum transceive time-out: 618 ms
* Extended length APDUs supported
* Maximum transceive length: 253 bytes
* Default maximum transceive time-out: 618 ms
MIFARE Classic support present in Android

# Detailed protocol information:
ID: 08:F7:EE:DD
* Random ID
ATQA: 0x0100
SAK: 0x20
ATS Historical bytes: [none]

--------------------------------------

